Security Blinds 
SecurTM security blinds
With the appearance of conventional vertical blinds, the Secur system incorporates tempered steel rods within extruded
aluminium blades and a patented locking mechanism thus preventing break-ins and protecting against ram raids, bomb
blasts and explosions.
Introduction Secur is a British
designed and patented product.
In addition to the highest standard of
security, Secur has an aesthetic,
professional design, which gives
protection without the feel of being
caged-in and blends in to create a
safer and more pleasant
environment in which to work and
live.
Secur looks and performs much like
a conventional vertical blind. The
blades can control sunlight, be
easily opened for ventilation and be
turned to allow for complete privacy,
sound insulation and thermal
insulation, thus helping the
carbon footprint of the building.
The blinds are unobtrusive and do
not detract from the look of the
building. Secured on the inside of
the building, into the window reveal
or face ﬁtted, they allow access for
cleaning and emergency egress.
Applications Typical applications
are in commercial premises, police
facilities, health facilities such as
surgeries, dental practices and
pharmacies, ﬁnancial organisations
such as banks, local government
buildings such as ofﬁces, town halls,
cash collecting sites and libraries;
residences, education premises
such as schools and colleges, and
information and control centres.
The system may be used with any
style or period of architecture, for
both new build and retroﬁt projects
and for Grade 1 and 2 listed
buildings.
Authority Secur complies with
local authority planning regulations
which may restrict the use of
external blinds and shutters.
It has received the Sold Secure
Gold Standard and exceeds the
requirements of BS 7950 for window
security and European Standard
ENV 1627 Grade 3. Secur blinds
are Secured by Design licence
holders endorsed by The
Association of Chief Police Ofﬁcers
(ACPO).
DESCRIPTION
Secur is installed internally and is
offered in a number of formats
including casement, horizontal
sliding or ﬁxed frame units. They are
made to measure for most sizes of
windows and doors.
Composition, manufacture
Secur comprises an inner and outer
frame. Aerofoil shaped aluminium
blade reinforced by tempered steel
rods retained in a perforated channel
at the head and foot comprise the
form of the blind. The casement
version is hinged with stainless steel
hinge pins located in steel hinge
blocks with double oilite bushes.
The horizontal sliding unit has steel
box interlocking sections and anti-lift
steel plates. All versions have locking
bars and lockable shoot bolts.The
steel outer frame is secured into the
substrate of the building using ﬁxings
normally 150 mm long. In doing so,
the blinds become an integral yet
immovable part of the building.
Shape Although square or
rectangular by ‘ﬂying-past’ an
opening, they are able to
accommodate arched features etc.
Dimensions Most situations are
resolved at survey; blades are
86 mm wide operating at 75 mm
centres.
Appearance Blinds are available in
most RAL powder coated ﬁnishes.
PERFORMANCE
Explosion Secur has been tested
and proved highly effective in
mitigating the effects of bomb blasts
and therefore provides a solution to
protect personnel and internal property
from terrorist or industrial explosions.
In the event of an explosion, the
blinds, in conjunction with
anti-shatter ﬁlm automatically snap
shut, preventing the ingress of ﬂying
glass and debris.
Light The full gloss ﬁnish will
borrow light; when closed Secur
acts as a black-out blind.
MAINTENANCE
Cleaning A simple wipe-down will
maintain appearance.
ECONOMICS
Guarantees Secur carries a full
10 year warranty.
SERVICES
The company offers a complete
design, manufacture and installation
service. The company's customer
satisfaction rating is 92%. In addition
the company use its own installation
teams to ensure the integrity of the
product is complemented by the
integrity of the installation.
REFERENCES
Security Blinds is the trading arm of Eruma Security International Ltd
Security Blinds 
2 St Hubert’s \Close
Gerrrards Cross
Bucks 
SL9 7EN
Tel: +44 (0)7779 015119
Email:
info@securityblinds.co.uk
Website:
www.securityblinds.co.uk
Technical Literature:
Illustrated brochure
20080868.indd 1
19/09/2007 22:07:39